**ZAŁĄCZNIK 1B**

DA.381.5.2025

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1** |  | **The Reflecting Pool** |  |  |
| 1.1 | 01 | Single Channel HD Playback System w/ Stereo EQ - BVS  stock |  |  |
| 1.2 | 01 | Custom Rigid Rear Projection Screen, frameless - 213x160cm, steel rope suspension - BVS |  |  |
|  | | |  |  |
| **2** |  | **Incrementation** |  |  |
| 2.1 | 01 | Custom Trigger Box w/ custom Engineering - BVS Stock |  |  |
| 2.2 | 02 | Custom 2" x 8 digit LED display - BVS Stock |  |  |
| 2.3 | 02 | Video Player w/ custom video load - BVS Stock |  |  |
| 2.4 | 02 | CRT Monitor w/ shelve console - BVS Stock |  |  |
| 2.5 | 02 | Loudspeaker - BVS Stock |  |  |
| 2.6 | 01 | Composite BNC Video Cable - BVS Stock |  |  |
| 2.7 | 01 | RVA Audio Cable - BVS Stock |  |  |
|  | | |  |  |
| **3** |  | **The Veiling** |  |  |
| 3.1 | 01 | Two Channel HD Playback System w/ Stereo Audio Decoder - BVS stock |  |  |
| 3.2 | 01 | Custom Designed Veils and Hanging Hardware w/ full set of spares - BVS stock |  |  |
| 3.3 | 01 | Custom Veils (Back UP) - BVS stock |  |  |
|  | | |  |  |
| **4** |  | **The Greeting** |  |  |
| 4.1 | 01 | Single Channel HD Playback System w/ Stereo EQ - BVS  stock |  |  |
| 4.2 | 01 | 4:5 vertical projection screen 284x243cm, custom made, image size 274x233cm, wall fixing - BVS stock |  |  |
|  | | |  |  |
| **5** |  | **Four Hands** |  |  |
| 5.1 | 01 | Four Channel Playback w/ Synch w/ Turn Key Authoring -  BVS Stock |  |  |
| 5.2 | 04 | Custom Framed 10,4" LCD Screens w/ Accessories mounted on custom shelve fabrication - BVS stock |  |  |
| 5.3 | 02 | Spare screen glass - from BVS |  |  |
| 5.4 | 02 | Spare screen controller - from BVS |  |  |
| 5.5 | 04 | 40' DC Extension Cables - BVS stock |  |  |
|  | | |  |  |
| **6** |  | **The Quintet of the Astonished** |  |  |
| 6.1 | 01 | Single Channel HD Video File and Turn-Key Playback Unit - BVS stock |  |  |
| 6.2 | 01 | Rear Projection Screen w/front frame bezel. 244 cm w x 137 cm h image size - BVS stock |  |  |
|  | | |  |  |
| **7** |  | **Anima** |  |  |
| 7.2 | 03 | Three Channel SD Playback - BVS stock |  |  |
| 7.3 | 02 | Custom Framed 17" LCD Screens w/ Accessories and spare components -BVS-stock |  |  |
|  | | |  |  |
| **8** |  | **Ascension** |  |  |
| 8.1 | 01 | Single Channel HD Playback System w/ Stereo EQ - BVS stock |  |  |
|  | | |  |  |
| **9** |  | **Interval** |  |  |
| 9.1 | 02 | Two Channel HD Playpack System w/ Custom Show Control plus spare system - BVS stock |  |  |
|  | | |  |  |
| **10** |  | **Pneuma** |  |  |
| 10.1 | 01 | Three Channel HD Playback w/ Warping/Mapping  Technology ans Audio Processing - BVS stock |  |  |
| 10.2 | 03 | Projector 4:3, 6500 ANSI, lens 1,34-1,74:1, DLP,  projection design, 1400x1050px, spare lamps - BVS |  |  |
| 10.3 | 03 | Mounting Head BVS-stock |  |  |
| 10.4 | 03 | Projector bracket - BVS-stock |  |  |
| 10.5 | 03 | Custom corner mounts - BVS-stock |  |  |
|  | | |  |  |
| **11** |  | **The Crossing** |  |  |
| 11.1 | 01 | Two Channel HD Playback System w/ Stereo Audio  Decoder - BVS stock |  |  |
| 11.2 | 01 | Custom Double Sided Projection Screen "The Crossing", 4 meters high - from BVS |  |  |
|  | | |  |  |
| **12** |  | **The Messenger** |  |  |
| 12.1 | 01 | Single Channel HD Playback System w/ Audio processor - BVS stock |  |  |
| 12.2 | 01 | 5:7 Vertical Projection Screen 428x306cm - custom made image size 427x258cm, steel rope suspension |  |  |
|  | | |  |  |
| **13** |  | **Room For St. John of the Cross** |  |  |
| 13.1 | 01 | Two Channel HD Playback System w/ Stereo Audio  Decoder - BVS stock |  |  |
|  | | |  |  |
| **14** |  | **External Rooms** |  |  |
| 14.1 | 01 | Single Channel HD Playback System w/ Audio processor -  BVS stock |  |  |
| 14.2 | 01 | 9:16 Vertical Projection Screen 510x291cm, - custom made, Aluminium frame 50x50mm, black matt, image size 500x281cm, steel rope suspension, from BVS-stock |  |  |
|  | | |  |  |
| **15** |  | **Gleb / Madison / Sharon** |  |  |
| 15.1 | 03 | Single Channel HD Playback System - BVS stock |  |  |
|  | | |  |  |
| **16** |  | **Earth Martyr, Air Martyr, Fire Martyr, Water Martyr** |  |  |
| 16.1 | 01 | Four Channel Playback w/ Synch w/ Turn Key Authoring - BVS Stock |  |  |
|  | | |  |  |
| **17** |  | **Three Woman** |  |  |
| 17.1 | 01 | Single Channel HD Playback System - BVS stock |  |  |
|  |  |  |  |  |